Copy the vertex information in a variety of ways.
The acquisition of the index of the vertex, use instead of "TMC-OBJ Converter" "for Blender TMC (PC) Importer".
It should be noted that the index other comma-separated, you can also specify a range as 10-15.

● Perp. Mode
Move the vertices only in a direction parallel to the normal. The amount of movement, will be defined by a cylinder which is determined from the coordinates and the normal of the vertices of the Source and Destination.
It is similar to the Blender of shrink-wrap, but there looks for the nearest surface without using the normal information.

● Update History

2016.2.19.1
- To create in order to make the appropriate undertones Reference of ABC Transformer, for the time being the public

2016.2.23.1
- Vertex of the selection method for Blender TMC (PC) Importer conform to the specification change
- Clipboard monitoring, other than the correct index list of the format was so can not paste in the button
If the index list is not correct, it was so Copy Vertices Data button is disabled
Copy a smoothing operation performed on the boundary of the vertex was also applied to the normal as well as the apex
· Automated Transformation was to perform a smoothing on the boundary of the vertices that you want to copy even if you do not perform the
Fixed an issue where · Abort button does not work
- At least one copy item was not allowed to press the copy button if it is not selected
• The UI was to fine-tune
- Was to display an error if the index of non-existent vertex is specified

2016.2.25.1
Objects that do not have a vertex was so as not to display
• The object of the skin was to be displayed with the "(Skin)"
• When reading the TMC, it confirms the Source if Destination, Destination if Source,
If it is not loaded, yet is object number of objects and vertices that are selected to match was present,
It was set to a state in which the object is selected
When you copy a part of the vertex-, add an option that does not perform a smoothing to the apex of the portion corresponding to the boundary of the mesh to be copied
- A copy of XYZ add Perp. Mode

2016.2.26.1
• In the index list was to be able to select all by pressing Ctrl + A
The automatic generation of regular expression, was not allowed to press the Copy button as long as the correct index has not been input
• In the same way, the correct index was not allowed to press the Paste button as long as that does not exist in the clipboard
· Variable implementation of the Number of Vertices function

2016.2.27.1
- A lot of dealing with the index and modify the response is extremely slow problem
- Fixed an issue where the executable file name had become ABC Transformer.exe

2016.2.28.1
· Source and fix the problem either its children the radio button and XYZ check box when it is not open was not in conjunction with the Destination
· Add the UV of the copy function
· Boundary changes to the more natural the definition of the (boundary)
Object the abolition of the function to perform the processing for all (on some use can not think, it is determined that confuse the user there is a limit to the use)
- Change the layout of UI
· UV copy function and implement automatic deformation of UV
· Boundary smoothing of was to choose individually in the XYZ and UV

2016.2.28.2
- The processing performed with respect to the normal to be performed even to the tangent
- A tangent was to be orthogonal with respect to normal

2016.2.28.3
Even-normal only a copy of the so as to perform a smoothing of the boundary

2016.2.28.4
- Fixed an issue where an error if you try to convert the TMC is displayed with the weight of the binary32
· Fixed an issue UI has become a not normal after the error display

2016.2.28.5
Error displayed when you do not appear as "finished"

2016.3.1.1
And conversion adds the ability to copy the affine transformation that least squares fit to the clipboard
- Adds the ability to run the affine transformation
• The automatic relocation at the time of the UV, is close enough to two points on the UV of interest was to determine the connectivity is regarded as of the same point

2016.3.1.2
- Affine correction because there was intended as the different parts to the format accepted as conversion parameters
- Fixed an issue that has been displayed with Vertex to meaningless part of the window
· XYZ at the time of automatic conversion of, close enough to two points on the XYZ was to determine the connectivity is regarded as the same point

2016.3.1.3
• When automatic conversion of XYZ Fixed an issue where the error is displayed on the
· XYZ close enough to two points on the XYZ in smoothing was set to determine the connectivity is regarded as the same point

2016.3.1.4
Right display of · TMC path Fixed an issue that was not stable
· In the automatic placement of UV, it was to be able to select the method of determining the connected component
(For 2016.3.1.1 previous methods and the subsequent method has been found that it is advantages and disadvantages)
Label of automatic deformation of UV is, fix the problem UV was invalid display as long as you do not take effect even four
Of · UV of smoothing label fix is ​​still in was the problem of invalid state

2016.3.3.1
· Boundaries and that are duplicated on XYZ is to perform the processing is regarded as the boundary

2016.3.3.2
· Swap Vertex is also one in the UV of Automated Transformation in Set mode when you run without check
Fixed an issue where there is an error is displayed

2016.3.3.3
And re-modification of 2016.3.3.2

2016.3.4.1
• For parameters of each vertex of the TMC to be output, the standard value if it is a NaN
And it is replaced (normal, tangent x-axis unit vector, others zero).

2016.3.7.1
Fonts to be displayed has not rely on environment
Tools startup in the "Drag and drop a TMC file." And was to be displayed

2016.3.8.1
- As long as the affine transformation in the case of manual input, modify the same conversion problems that applied have been the transformation of space by mistake to the normal line of the conversion
Abolish the specifications Source can not drop in-affine transformation mode of
• If the affine transformation mode file in the Source at the time has been dropped, it was to switch to normal mode
- Fixed an issue where the Paste button in 2016.3.7.1 had no longer function

2016.3.16.1
Trying to copy the weight of the · binary32 to and correct the error has been displayed problem
- Was to be able to copy the tangent vector independently
· Swap Vertex Set Fixed a bug that Boundary Smoothing does not work in
• Even if the vertices do not specify the UV to the selection method there is no UV and correctly modify the vertex can not be selected problem
- Change it to something easy to understand the error message when bone fails to reason insertion of the mesh, such as missing
· Swap Vertex Set in Automated Transformation fix a problem that can not be executed pattern exists
- Was to use the transposition cofactor matrix rather than a transposed inverse matrix as a transformation matrix for normal
(It is the result in most cases the same, cofactor matrix will be determined even for matrix that does not have an inverse matrix)

2016.3.17.1
· XYZ: UV = 10: 0 and fix because the error level was a mistake twice minute on a logarithmic scale in 0:10

2016.3.18.1
Index of the text box has to be able to drop a text file to